

**POLYETHYLENE HOSE**

The drip tubing shall be manufactured of polyethylene and 2% black for UV resistance. The drip tubing shall be available with the standard blue stripe, and certain models shall have the option of a white stripe, or lavender (effluent) stripe.

The drip tubing shall be model number \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ and shall be manufactured by The Toro Company, Irrigation Division, based in Riverside, California, USA.

**Performance Specifications**

Maximum length of run

* T-EHW0437-100

1,000’ @ 161 psi

* T-EHD0437-010

100’ @ 161 psi

* T-EHW1645-010

100’ @ 61 psi

* T-EHW1645-050

500’ @ 61 psi

* T-EHD1554-050A

500’@ 77 psi

* T-EHD1645-050A

500’@ 61 psi

* T-EHD2057-050A

500’@ 59 psi

* T-EHD2667-066A

660’@ 53 psi